

How to cut the RAM for FUS camera


1. first check whether the RAM is allocated to FUS camera . the below pic is correct to allocated (the solution way is only for 64bit and 16G RAM)



1. Click Start button and input “CMD” and then right click run as administrator



1. Please copy this sentence as the below picture to the interface and click enter ,then it will show successfully (The sentence:bcdeditspacebar/setspacebar{current} spacebartruncatememoryspacebar0x3a0000000enter Notice the space bar)



4.then restart the computer and analyzer